===============================================================================
Intel(R) Server Platform Integrated BMC Firmware Release Notes
===============================================================================

INTEL(R) Server Boards and Systems 
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA


===============================================================================
DATE:       July, 2026
TO:         Intel(R) Server Board D50DNP

SUBJECT:    Integrated BMC(R) firmware 3.02-6 release notes

===============================================================================
LEGAL INFORMATION
===============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppel or otherwise, to any intellectual
property rights is granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not
provide any license, express or implied, by estoppel or otherwise, to any
such patents, trademarks, copyrights, or other intellectual property rights.
Intel products are not intended for use in medical, life saving, or life
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.


Intel is a registered trademark of Intel Corporation.


*Other names and brands are the property of their respective owners.


Copyright (c) 2026 Intel Corporation.

===============================================================================
ABOUT THIS RELEASE PACKAGE
===============================================================================
Offline programming images:
dnp-signed-OBMC-egs-3.02-6-gc132f5-075b0000-pfr-full.ROM

Out Of Band(OOB) update images: 
dnp-signed-OBMC-egs-3.02-6-gc132f5-075b0000-pfr-oob.bin

Built from git revision:
OpenBMC:    COMMUNITY_HASH=075b81bea9694df7e1096da74b737645e1d2ee77
Meta-Intel: INTEL_HASH=c132f5b6133a0d0cd3ab8cef699bd7264f52a363

REVISION INFORMATION RETURNED BY GET DEVICE ID COMMAND:

DNP Product ID:     0x00ac
Device ID:          0x23
Manufacturer ID:    0x000157
Firmware Revision:  egs-3.02-6-gc132f5-075b0000

BMC PFR SVN: 1

SHA1 checksum:
dnp-signed-OBMC-egs-3.02-6-gc132f5-075b0000-pfr-full.ROM c04deb3ceba5ece98c854f7dc0543375448a2686
dnp-signed-OBMC-egs-3.02-6-gc132f5-075b0000-pfr-oob.bin 00f745e23fa4fdbc9e34432052cb4d19880766b5

Embeds firmware files for the following components:

Power Supplies:
2100WT  S2: 128.3.3
2100WT  S3: 128.4.4
DPS-1300AB-53A  S0F: 0.1.7
DPS-1300AB-53A  S0F: 128.4.16
DPS-1600AB-69A  S0F: 0.0.5
DPS-1600AB-69A  S0F: 128.3.13
DPS-2700CBA  S: 128.0.45
DPS-900AB-5  01F: 128.14.14
PSSF132202A  00: 128.5.33
PSSF132202A  01: 128.5.33
PSSF132202A  02: 128.5.33
PSSF132202A  03: 128.5.33
PSSF132202A  04: 128.5.33
PSSF132202A  05: 128.5.33
PSSF132202A  06: 128.5.33
PSSF132202A  07: 128.5.33
PSSF132202A  08: 128.5.33
PSSF162202A  00A: 128.9.75
PSSF162202A  01A: 128.9.75
PSSF162202A  02A: 128.9.75
PSSF162202A  03A: 128.9.75
PSSF162202A  04A: 128.9.75
PSSF162202A  05A: 128.9.78
PSSF162202A  06A: 128.9.78
PSSF162202A  07A: 128.9.78
PSSF162202A  08A: 128.9.78
PSSF162202A  09A: 128.9.78
PSSF162202A  11A: 128.9.78
PSSF162202A  S3: 0.9.55
PSSF162205A  00A: 128.4.22
PSSF162205A  01A: 128.4.22
PSSF162205A  02A: 128.4.22
PSSF162205A  03A: 128.4.22
PSSF162205A  04A: 128.4.22
PSSF162205A  05A: 128.4.22
PSSF162205A  06A: 128.4.22
PSSF162205A  S3A: 128.2.6
PSSF212201A  00: 128.3.12
PSSF212201A  01: 128.3.17
PSSF212201A  02: 128.3.17
PSSF212201A  03: 128.3.17
PSSF212201A  04: 128.3.17
PSSF212202A  00A: 128.5.8
PSSF212202A  01A: 128.5.8
PSSF212202A  02A: 128.5.8
PSSF212202A  S2:  128.3.3
PSSF212202A  S3:  128.4.4
PSSF222201A  01: 0.0.24
PSSF222201A  S3: 128.0.20
PSSF222201A  S4: 128.0.33
PSSF302201A  00A: 128.7.8
PSSF302201A  00A: 128.7.8
PSSF302201A  01A: 128.8.9
PSSF302201A  01A: 128.8.9
PSSF302201A  S2: 128.3.3
PSSF302201A  S2B: 128.6.6
PSSF302201A  S3:  128.7.8
PSSF302201A  S3: 128.7.8
PSSF302201B  01A: 128.8.9
S-1100ADU00-201  00: 129.1.54
S-1100ADU00-201  01: 129.1.54
S-1100ADU00-201  02: 129.1.54
S-1100ADU00-201  03: 129.1.54
S-1100ADU00-201  04: 129.1.54
S-1100ADU00-201  05: 129.1.54
S-1100ADU00-201  S3: 129.1.54

Hot Swap Backplane:
FCP V2 HSBP: 2.05

Retimer:
dnp_retimer_fw_2u_riser V1.25.0
dnp_retimer_fw_accl_riser V2.8.32
dnp_retimer_fw_cbb V2.7.0

PDB FW version: v06

FRU File:
DNP Baseboard FRU file version:0.09
DNP Systemboard FRU file version:0.1


Sysfwupdt Utility: V16.0.12

===============================================================================
IMPORTANT NOTES
===============================================================================
1. Starting from BMC1.30 + CPLD 3.0, the behavior of updating BMC with Immreset
   switch has changed as below due to the latest design change:
      Sysfwupdt -u bmc.bin ImmReset
    
      Old behavior: Only BMC reset, PCH keeps alive(the system will not reset)
      New behavior: Both BMC and PCH will reset(the system will reset)

2. Users need to restore BMC full factory default state if the original BMC
   version is lower than 1.34, otherwise, some functions like power will be
   impacted by rwfs filesystem getting almost full (HSD: 15012405799).
   To restore factory defaults, in the Embedded Web Console navigate to 
   Server Diagnostics -> System Defaults -> Restore Default - Full -> Restore

3. Users need to clear post code via Redfish if the original BMC version is
   lower than 1.52, otherwise, Generate System Debug Log function might be
   impacted by post code format mismatch (HSD: 15012990256).
   Redfish Command: (POST method)
   https://<BMC_IP>/redfish/v1/Systems/system/LogServices/PostCodes/Actions/LogService.ClearLog

4. Virtual KVM over HTML5 feature is now available as part of the Advanced
   Server Management functionality that requires an optional product license
   key (iPC ADVSYSMGMTKEY).

5. Options to upload Intel(R) VROC Activation License Key are added to BMC
   starting from version 1.53.
   
6. Starting from BMC version 2.15-1, the Retimer FW update function is disabled.
===============================================================================
INSTALLATION PROCEDURE
===============================================================================
WARNING:  It is very important to follow these instructions as they are written.
Failure to update using the proper procedure may cause damage to your system.

The recommended method is to run startup.nsh file to update all FW components in 
proper order.

User also can update BMC using one of the following methods.

  A. Using sysfwupdt utility in UEFI environment

     1. Unzip the contents of the update package and copy all files to the root 
        directory of a USB flash drive
     2. Insert the USB flash drive into available USB port on the system to be
        updated
     3. Power on the server and load the uEFI shell. Press <Esc> to terminate
        autostart.
     4. Run UpdBMC_DNP.nsh script. After the script completes loading the BMC
        firmware file into the staging area, restart the server to begin
        the programming process. The status LED will blink green/orange for
        about 10 minutes.
     5. Once the BMC update process has successfully completed, the system will
        boot automatically. The whole process takes around 15 minutes.

  B. Using BMC Web Console
  
     1. Open BMC Web Console and login
     2. Go to Configuration > BMC Firmware Update
     3. if desired, select "Recovery" and/or "Reset Immediately" checkboxes
     4. Choose the File (dnp-signed-OBMC-egs-2.20-0-g2ce4c5-39e80000-pfr-oob.bin)
     5. Click "Upload"
     6. BMC will be updated on the next reboot (if "Reset Immediately" checkbox
        was not selected).

===============================================================================
KNOWN ISSUES/WORKAROUNDS/REQUIREMENTS
===============================================================================

N/A

===============================================================================
CHANGES
===============================================================================

egs-3.02-6-gc132f5-075b0000:
Defect: Harden NFS mount command execution (#42)
Defect: [DNP][FCP] Enhance support for Micron, Phison, and Solidigm NVME Devices

Defect:[BTS-51588] DNP LC(4 node) KDK PSU redundancy occurs during the AC power cycle
Feature:Fix BDBA CVEs #686
Feature:Upgrade linux kernel to 5.15.202 for security fix #685
Feature:Fix CVE for zlib in storelib7 #52

Feature: Implement NIC temperature sensor

egs-2.94-0-gee0a08-075b0000
Feature: [CCB 4858] Add support for verifying v2c license files using multiple public keys.

Feature: Update MDSG cert for EWS custom

Defect: [DNP][FCP] Micron Device Fails to Enumerate Sensor
Defect: [DNP][FCP] Phison NVME Device Fails to Enumerate Sensor on FCP and DNP

Defect: [DNP] Phison NVME Device Fails to Enumerate FRU
Feature: Dump the current server status in System Debug Log (#51)

Defect: [BMCFW-9][FCP] HSBP FW update
Feature: Update PSU fw version 20250811

Feature: reduce duplicated MultiNode-related journal log for dbus-sensors #115
Feature: Upgrade linux kernel to 5.15.193 for security fix #663

Defect: [BTS-50700][DNP]Redfish PCIe event show incorrect BDF location
Defect: [CCB 4856]Change the raw data in SEL log
Defect: [DNP][LC] fan sensor threshold going low issue

egs-2.71-0-g778b0a-53400000:
Defect: The logically dead code from Coverity scan. (#11)

Defect: [BTS-49197][DNP] [2U-ACCL]BMC FRU Service Abnormal During Power Cycling Test
Defect: [BTS-49201][DNP] [2U-ACCL]BMC PLDM Device Redfish Path Lost With X710-DA2 During Power Cycling Test
Feature: Update PSU fw version 20250515

Defect: [DNP#50413] EWS Redfish event 0147 Post Error Code message is not matched with Error manager 0147 error message.
Defect: [FCP#50412] EWS Redfish event 0147 Post Error Code message is not matched with Error manager 0147 error message.
Defect: cpusensors were missing if the BMC time moved backward after synchronizing with the PCH RTC.

Defect: BTS-49035 BMC FRU randomly lost during power cycle with Micron 7450
Defect: [BTS-33809]Members of redfish path "/redfish/v1/Systems/system/PCIeDevices" are incorrect
Defect: [BTS-35850]Members of redfish path "/redfish/v1/Systems/system/PCIeDevices" are incorrect
Defect: [BTS-49035] BMC FRU randomly lost during power cycle with Micron 7450 MAX 400GB M.2 PCIE configure
Defect: [BTS-49197] BMC FRU Service Abnormal During Power Cycling Test
Defect: [BTS-49205] BMC Occur Recovery During Power Cycling Test
Defect: [BTS-49518] If the UUT with an E810 network card, after executing reset -c, the Riser fru will not be able to read.
Feature: Follow Intel DSG PSU FW vesion change to update the Delta PSU fw file

egs-2.42-2-g4940a9-39e80000:
Feature: Update MDSG cert for EWS custom

Defect: [BTS-47916/47920] All PSU model versions require the latest PSU firmware image to be implemented into the BMC code

Defect: [BTS-48003/48002] The storage information is not displayed on the EWS storage information page
Feature: Add Phison NVME FRU and temp sensor support
Feature: Update PSU fw version
Feature: [FCP] HSBP FPGA fw version update to v2p4

Defect: Release note build error.
Defect: [BTS-33812][14022512564] DNP ACCL modules lost many sensors after FW upgrade

Defect: [15015938808][EGS]BMC should delete "reset BIOS to default" action in redfish output
Feature: Add PSU 2nd source Delta 1300/1600 support
Feature: Add Voltage In sensor for DSG PSUs
Feature: Update PSU fw version

Defect: [DNP#0142] NVIDIA H100 80GB FRU randomly lost during power cycling test.

egs-2.20:
Defect: [DNP][14022512564]DNP ACCL modules lost many sensors after FW upgrade
Defect: [DNP][22019826638] Adcsensor failure and it caused BMC recovery by PFR. (BMC MAC addresses changed to random)

Defect: [DNP#0143][ACCL]BMC will randomly trigger ACCL RTM FW update during QRC test
Defect: [DNP#139/FCP#133]The CA certificate will be cleared after updating BMC 2.12
Defect: [FCP#126] Redfish Logs records fan fault recovery event before event before the obstruction is cleared

Defect: HSD[22019335902]BMC does not write the system tracking and real time data into PSU black box

Defect: [DNP#123/FCP#118]Storage Information Command Data Response Information Missing.

Defect: [DNP#121/FCP#116]SDPtool NICINFO command data request response is abnormal.
Defect: [DNP#131] 2700W PSUs Will Lose All PSU Sensors With 2.07 BMC on DNP
Defect: [FCP#126] Redfish Logs records fan fault recovery event before event before the obstruction is cleared
Feature: Update CBB FPGA to 1.2 and CBB Retimer to 2.7.0
Feature: [DNP] Update ACCL retimer fw to 2.8.32

Defect: [DNP#124/FCP#119] Redfish can display NIC information with wrong paths

Defect: BMC returns 0x00 completion code when user modifies FRU field with over 32 characters.
Defect: BMC will record repeated PSU predictedfailure assert/deassert log while PSU encounters issue
Defect: Coverity scan issue
Defect: [DNP#0126] BMC cannot detect OAM FRU after upgrade BMC 1.95-0
Defect: the service xyz.openbmc project.pldmd.service has exited

Defect: [DNP#102/FCP#97]The system can enable the Shutdown Policy via the IPMI tool even if it is not supported.

Defect: the service xyz.openbmc project.pldmd.service has exited

Defect: [DNP#89/FCP#85] The copyright information on the EWS needs to be updated
Defect: [DNP#98/FCP#93]Set BIOS Config via SDPtool Will Cause Service Bmcweb.service to Crash
Defect: the service xyz.openbmc project.pldmd.service has exited

Defect: [DNP#82/FCP#78]SUT Unable to Perform FW Update Via Local Image File
Defect: [FCP] There is an error in 2100W PSU dual rotor fan definition

egs-1.95:
Defect: [DNP#85/FCP#80]Password cannot be saved and the User even be cleared with BMC 1.94-0

Defect: [DNP#73]Redfish detected non-existent disk under EWS when install multi-node system.
Defect: [DNP#81/FCP#77]The "Network Privileges" of user page cannot be modified if log in EWS with Chinese.
Feature: [CCB3721] Dump PSU Blackbox data in System Debug Log (#609)
Feature: [FCP] HSBP Fpga fw version update to V2p3

Defect: Can't set username and legal password in the BIOS setup menu at the same time.
Defect: [DNP#71/FCP#75] Wrong Chinese warning message when the password does not meet the complexity.
Feature: Add LC 3000W Titanium 01A 9.8.128 PSU firmware
Feature: Dump PSU Blackbox data in System Debug Log (#47)

Defect: Not detected Samsung PM9A3 M.2 Temp sensors via EWS
Defect: [DNP#63/FCP#65]There is one abnormal event “Service phosphor-ipmi-host.service has exited unsuccessfully”
Defect: [DNP#67/FCP#72]System debuglog's BIOS changed attribute list will always overwrite the newest entry
Defect: [DNP#70/FCP#74] Some SUT download events from EWS in different formats
Feature: Support MDSG and new DSG cert for EWS custom
Feature: [15010870327] [Feature improvement][LocalImage] The Local image does not support writ for ima/img files

Defect: [15014205307] Redfish host IP address is not filled in SMBIOS table after AC cycle.
Feature: [CCB4826] Add support for new VROC Key


Defect: [DNP#60/FCP#63] The non-allowed password of BMC user still can be saved under BIOS setup
Defect: [DNP#64/FCP#67] The popup error warning of NM Configuration isn't translated to Chinese.

Defect: [DNP#47/FCP#56]Sometimes system lose some sensors during AC/DC cycles stress
Defect: [DNP#49] Recommend graying out "Force-enter BIOS setup" button in "provision host disabled" KCS mode.
Defect: [DNP#58/FCP#60] fansensor.service exited events generated after FRU information is updated.
Defect: [DNP#61] Not Detected 7450 MAX U.2 SSD sensor.
Defect: [FCP] DIMM sensor will not trigger any threshold event before ThermTrip


Defect: [DNP#57/FCP#59] System doesn't reboot automatically after generating IERR event.
Defect: [FCP#53/DNP#43]AD user unable to login EWS when auth over ssl is enabled
Defect: [FCP#61] The PN/SN of HSBP is wrong on Redfish URL /redfish/v1/Systems/system/Storage/1


Feature: [CCB4795] [BMC] Add temperature sensor for E810 network card
Feature: [CCB4796] Add temperature sensor for ATS M1/M3 card

egs-1.81:

Defect: The defect divide_by_zero from Coverity scan.
Defect: [FCP#54/DNP#45] Unknown chassis installed events generated after AC Cycle

Defect: (klocwork) Operands in a bitwise operation have different size
Defect: [15014205307] Redfish host IP address is not filled in SMBIOS table after AC cycle.

Defect: Redfish response "202 Accepted" even though PATCH the illegal fru value.

Defect: FSC didn't work after user modify the product product name of baseboard FRU
Defect: The thresholds of TI 900W PSU can't reach expectations.
Defect: [15014177258] EWS only show few sensor after changing fru product name

Defect: After AC cycle can't get Arc card fw version (#5)
Defect: Sensor reading of "Exit Air Temp" is extraordinarily high on BMC web of DNP LC system
Defect: [DNP#15/FCP#14] Some EWS pages is abnormal after pressing sequence buttons
Defect: [DNP#32/FCP#32] The details of EWS NM Configuration doesn't match its profile after we sort the NM policies.
Feature: Expose temp sensors of Midplane

Defect: [15010915549] LDAP user unable to login EWS when auth over ssl is enabled
Defect: [DNP#33/FCP#33]The Email Alert function through SMTP from EWS is fail.
Defect: [DNP#24/FCP#20]There are Multiple Sensors Missing on EMR CPU
Defect: Using EMR cpu, BMC would occur kernel panic.

Defect: Fail to check Mellanox MCX623106AN-CDAT ‘s FRU info via Redfish.
Defect: [DNP#20/FCP#16]The system event logs of baseboard "Board serial number" and "Chassis serial number" is incorrect.
Defect: [DNP#26/FCP#22] First time to trigger an OEM Add SEL Entry command but there are 2 events added

Defect: System will lose VROC Upgrade Key after BMC reset
Feature: [CCB3721] Log any BIOS setting change in System Debug Log

Defect: [2103657597]Service system-watchdog.service has exited unsuccessfully
Defect: [2103659285] Storage information page is abnormal after press the sequence button.
Defect: [BTS0011] Physical device information page is abnormal after pressing the sequence button
Defect: [BTS0011] The “Enable” of NM Configuration page doesn’t be clicked if user selects an enabled Node Manager policy.
Defect: [BTS0015] Some EWS pages is abnormal after pressing sequence buttons
Defect: [BTS009] The NVMe information of Redfish is abnormal with FCP R1212/R2208/R2224.
Defect: [BTS18]Password Complexity not keep High after BMC update
Defect: [BTS][DNP#23/FCP#19] Sysfwupdt cannot update CPLD with BMC : 1.70-0
Feature: Add Delta_DPS-900AB_PSU.json for DC 900W Delta PSU

Defect: (klocwork) base64String is not initialized (#15)

Feature: [CCB4793] Change VROC License key to node locking - Use new

Defect: There is no Advantest riser item under /redfish/v1/chassis

Defect: [15013360465][FCP] Expect no Storage tab if RAID not detected on system
Defect: [2103659285] Storage information page is abnormal after press the sequence button.

Feature: Support Advantest riser card FRU

Defect: [2103657804] BIOS ITK cap file cannot be updated via EWS
Defect: [2103658047] AD/LDAP Setting can’t be set to disable in EWS.

Feature: [FCP] HSBP Fpga fw version update to V2p2

Defect: [15013347489] Update AMC Fw total progress percentage value is wrong

Defect: [15013347495] it needs OS reboot to re-discover all AMC after updating PVC AMC firmware
Defect: [2103651949]Can't update Arctic Sound card (#7)
Defect: [2103658547]phosphor-ipmi-host.service failure during DC cycle test

Feature: [CCB3670] add ability to clear and set bios admin password from redfish interface (#394)

Defect: [2103654938][DNP LC OAM] OAM CBB_OAMX_PVC FRU and SDR lost
Defect: [2103658161] The EWS help information and warning message has some issues.

Defect: [2103658037] Supported RAID Levels in EWS Page Incorrect for MegaRAID 9540-8i RAID Card

Defect: [15013028475] When delete primary DNS server IP in IPv4 setting
Defect: [16018966304] BMC SEL log should contain both Error Code and
Feature: Add Get CBB Retimer Temp OEM command for SDP customer
Feature: Add Get Retimer Temperature reading

Defect: When adding different types of VROCkey, the utility tool cannot obtain the return value of the ipmid command.
Defect: [2103655071] BMC will crash when run script to write VLAN ID.
Defect: [2103657728] HBA card RS3P4GF016J cannot be detected on EWS storage page after connecting external storage array.
Defect: [CCB3759] Validate new entry RAID adapter Broadcom channel 9540-8i

Defect: Fixed raid level option error when multi-card
Defect: [15013024578] [EGS][CCB3768] Get VROC software key level via 0x30 0x9d should be restricted to KCS channel and only available in POST phase (#186)" (#188)
Defect: [15013069841] Fix the property 'LinkStatus' value is not as per DMTF schema (#392)
Defect: [176554][klocwork] 'value' is used uninitialized in this function

egs-1.53:
First Production Release 
Defect: PSU Fan Speed 2 sensor is no reading with the 2100W Titanium PSU
Defect: The ipmid command cannot be executed during the execution of the dump-jounal script.
Defect: [15012885574] Sensor warning triggered on PVC when reading is 0
Defect: [15013024578] [EGS][CCB3768] Get VROC software key level via 0x30 0x9d should be restricted to KCS channel and only available in POST phase (#186)
Defect: [15013036205] During BMC reset stress test, BMC automatically downgraded to backup version.
Defect: [2103657375] EWS customization bin file cannot be updated successfully.
Feature: Only update CBB retimer 1.27.12 for DNP SDP image
Feature: CBB retimer fw update to  1.27.12 (#69)" (#71)

Defect: Drop files to the page to upload license failed.
Defect: [2103655546] No sensor information is displayed on EWS with SDP BMC (#5)
Defect: [2103657530] After setting 2 alert destinations , it can not sent test mail successful.
Feature:Update ACCL FSC

Defect: Modify the 74h, 78h and 9ch cmd for VROC key, add 9dh cmd.
Defect: Modify the upload page of EWS for premium key.
Defect: [15012822478] Fan PWM Offset is 20 by default, which it should be 0
Defect: [CCB 3768] Support VROC Software Key, modify ipmid CMD 3eh 74h, 30h 9ch
Defect: modify license upload URL for premium
Feature: Add PSSF212202A.json for 2100W Titanium PSU
Feature: Modify SPI filter rule to change the erase way after recovery Description: (#541)
Feature: [CCB3768] add support of other type of key such as vroc (#6)

=============================================================================
REFERENCE MATERIAL
===============================================================================

[Integrated BMC Web Console User Guide for the Intel® Server Boards M50FCP and D50DNP]
https://www.intel.com/content/www/us/en/secure/content-details/733625/content-details.html
