================================================================================
DATE : July 2026
TO : Multi-Core Intel(R) Xeon(R) Processor-Based Server Platform customers
SUBJECT : BIOS Release notes
================================================================================
                           LEGAL INFORMATION
================================================================================

Information in this document is provided in connection with Intel Products
and for the purpose of supporting Intel developed server boards and systems.
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation 
may have patents or pending patent applications, trademarks, copyrights, or
other intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any such
patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (C) 2026 Intel Corporation.

================================================================================
                                                      ABOUT THIS RELEASE
================================================================================
Build Stamp: SE5C7411.86B.R01.02.0006
Build Date: May 10 2026
================================================================================
                                                      Supported Platforms
================================================================================

	DaneliPass	
		R01.02.0006_DenaliPass_EBG_EMR_PFR_prd.bin
		Checksum: 0x31694896
		SFID offset: 0x7D0024
		SFID value: 0xc11b425f

================================================================================
                                                      BIOS COMPONENTS/CONTENTS
================================================================================
Processors supported: 
		Xeon Scalable Family Processor

Microcode versions:
             CPUID                Version                Stepping 			 		
             m_87_c06f*           0x210002e0             EMR A*/R*
             m_10_806f8           0x2c000421             HBM B*
             m_87_806f*           0x2b000670             SPR E*/S*
             	 		 		
RSTeSataEfi:
		v9.0.0.2018
RSTesSataEfi:
		v9.0.0.2018
BIOSACM:
		Production,v1.1.A_PW
ACTM:
		Production,actm_emr_01.00.02_PW_prod_signed
SINIT:
		Production,v1.1.A_PW
VMDDxeEfi
		v9.0.0.2018
RSTeSataRaidEfi:
		v9.0.0.2018
AspeedVideo_2600:
		v8.01.11.02
BiosGuard:
		BIOSGuard_pc_2.0.218
SPS:
		SPS_E5_06.01.04.215.0
Production_PMCP:
		EBG_B0_PMC_FW_152.00.01.0021_Production
PCH PFR SVN:
		3
S3M_FW:
        s3m_fw_ProdEncr_ProdSigned_SESVN0x1_SVN0x1_REVID0x1e	
S3M_FW_EMR:
        s3m_fw_ProdEncr_ProdSigned_SESVN0x1_SVN0x1_REVID0x20
CFR_PUCode_EMR_A1:
		cfr_active_encrypt_signed_31000030
CFR_PUCode_EMR_MCC_R1:
		cfr_active_encrypt_signed_33000010
CFR_PUCode_E0:
		cfr_active_encrypt_signed_1e0000a0
CFR_PUCode_E2:
		cfr_active_encrypt_signed_1f0000a0	
CFR_PUCode_E3:
		cfr_active_encrypt_signed_19000070
CFR_PUCode_E4:
		cfr_active_encrypt_signed_3a000060
CFR_PUCode_E5:
		cfr_active_encrypt_signed_3b000040		
CFR_PUCode.MCC_S0:
		cfr_active_encrypt_signed_120000d0
CFR_PUCode.MCC_S1:
		cfr_active_encrypt_signed_18000070
CFR_PUCode.MCC_S2:
		cfr_active_encrypt_signed_39000070
CFR_PUCode.MCC_S3:
		cfr_active_encrypt_signed_38000060
CFR_PUCode.LCC_U0:
		cfr_active_encrypt_signed_15000090
CFR_PUCode.LCC_U1：
		cfr_active_encrypt_signed_37000030
CFR_PUCode_HBM_B0:
		cfr_active_encrypt_signed_130000c0
CFR_PUCode_HBM_B1:
		cfr_active_encrypt_signed_16000080
CFR_PUCode_HBM_B2:
		cfr_active_encrypt_signed_17000040
CFR_PUCode_HBM_B3:
		cfr_active_encrypt_signed_3c000060
TDX:
                TDX_1.5.28.04_PRODUCTION_SIGN
================================================================================
                                                      INSTALLATION NOTES
================================================================================

WARNING:  It is very important to follow these instructions as they are written.
Failure to update using the proper procedure may cause damage to your system.

The recommended method is to run startup.nsh file to update all FW components in 
proper order.

User also can update BIOS using one of the following methods.

  A. Using sysfwupdt utility in UEFI environment

     1. Unzip the contents of the update package and copy all files to the root 
        directory of a USB flash drive
     2. Insert the USB flash drive into available USB port on the system to be
        updated
     3. Power on the server and load the uEFI shell. Press <Esc> to terminate
        autostart.
     4. Run UpdBIOS_DNP.nsh script. After BIOS update file is loaded into the
        staging area, the server will be powered off with the system status LED
        blinking green/orange and the blue ID LED is solid on for about 10 minutes.
        During this time the system reprogramms the BIOS under control of PFR. 
     5. Once the BIOS update process has successfully completed, the system will
        reset automatically couple of times and finaly boot. The whole process
        takes around 15 minutes.

  B. Using BMC Web Console
  
     1. Open BMC Web Console and login
     2. Go to Configuration > BIOS/IFWI Firmware Update
     3. if desired select "Recovery" and/or "Reset Immediately" checkboxes
     4. Choose the File (XXX_UpdateCapsule_prd.bin)
     5. Click "Upload"
     6. BIOS will be updated on the next reboot (if "Reset Immediately" checkbox
        was not selected).
     7. Do *NOT* interrupt the BIOS POST during the first boot.

================================================================================
                                                      SVN_BYPASS Jumper
================================================================================
Platform does not allow flashing PFR-controlled PCH capsule with the security 
version number (SVN) lower then the SVN of the curently running FW. 
When BIOS SVN Downgrade jumper is moved from its default pin position (pins 1–2), 
it allows the BIOS firmware to be downgraded to a lower SVN. 

To use the BIOS SVN Downgrade jumper, perform the following steps:
1.	Power down the server module.
2.	Remove the server module from the chassis.
3.	Remove the riser assembly #2 from the server module. (See the Intel® 
	Server D50DNP Family Integration and Service Guide for details).
4.	Move the BIOS SVN Downgrade jumper (J14) from pins 1–2 (default) to pins 2–3.
5.	Reinstall the server module in the chassis.
6.	Power on the server module and boot into the UEFI Shell.
7.	Update the BIOS with the required image using the "-recovery" switch on
        the sysfwupdt.efi command line. Ex.: sysfwupdt.efi -u xxx.bin -recovery
8.	After BIOS update is successfully completed, power down the server module.
9.	Remove the server module from the chassis.
10.	Move the BIOS SVN Downgrade jumper (J14) back to pins 1–2 (default).
11.	Reinstall the riser assembly #2.
12.	Reinstall the server module in the chassis.
13.	Power on the server module. During POST, press <F2> to access the BIOS 
	setup utility to configure and save desired BIOS options.

================================================================================
                                                      IMPORTANT NOTICE
================================================================================
1. VT-D is enabled by default in this BIOS release. If you are still 
   using Windows Server 2019, please disable VT-D and Extended APIC or enable 
   “Limit CPU PA to 46 bits” to avoid BSOD under Windows Server 2019:
        Advanced ->Integrated IO Configuration -> Intel VT for Directed I/O (VT-d)
        Advanced -> Processor Configuration -> X2APIC 
        Advanced -> Processor Configuration -> Limit CPU PA to 46 bits
   VT-D and X2APIC are bundled, please disable X2APIC first when you want to 
   disable VTD.
2. Starting from BIOS version R01.01.0001 PFR Lock is enabled by default. User
   need to add "UpdateNvram" parameter during BIOS update to load the new default
   value of PFR lock. Alternatively manually set PFR Lock to Enable in BIOS setup
   after BIOS update.
3. Starting from BIOS version R01.01.0001 the default value for the "Volatile
   Memory Mode" parameter has changed from 2LM (2LM is removed) to 1LM due to
   silicon code change. User must add parameter “UpdateNvram” when updating
   BIOS from a version lower than R01.01.0001.
4. User must add parameter "-recovery" when updating BIOS to the version with
   higher SVN, otherwise online update will fail.
5. R01.02.0001 is the first version to support both Intel(R) Xeon(R) 4th and 5th 
   Gen Scalable procesors. The Security Version Number (SVN) was incremented to
   3 to differentate this release from previous versions and to prevent 
   accidental BIOS downgrade. If FW downgrade is required, refer to the 
   SVN_Bypass Jumper section. The "-recovery" and "UpdateNvram" parameters
   are required to update from R01.01.0005 or older versions. 
6. Incremented SVN in BIOS version R01.02.0001 prevents the main BIOS capsule
   and the BIOS customization capsule to be updated in one session. Update the
   main BIOS code first, reboot the system and after that update the BIOS
   customization capsule file. 
7. BIOS version R01.02.0001 enables "Manual Commit S3M FW CFR" and 
   "Manual Commit Pcode/Ucode CFR" options. Users need to add "UpdateNvram"
   parameter during BIOS update to load the new default values. Alternatively
   manually set default vlaue of "Manual Commit S3M FW CFR" or "Manual Commit
   Pcode/Ucode CFR" in BIOS setup after BIOS update.
8. BIOS version R01.02.0001 added "Auto" option for the "C1 Auto Demotion"
   parameter as default. Users need to add "UpdateNvram" parameter during BIOS
   update to load the new default value for the "C1 Auto Demotion" parameter
   or manually set "C1 Auto Demotion" to "Auto" after BIOS update.
9. BIOS version R01.02.0001 removed "10Mhz in I3C mode" option for the
   "I3C Clock Frequency" parameter. Users need to add "UpdateNvram" parameter
   during BIOS update to load the new default value for the "I3C Clock Frequency"
   parameter.
10. BIOS version R01.02.0001 added "Auto" option for the "SGX PRM Size"
    parameter as default. Users need to add "UpdateNvram" parameter during BIOS
    update to load the new default value for the "SGX PRM Size" parameter or
    manually set "SGX PRM Size" to "Auto" after BIOS update.
11. 5th Gen Intel(R) Xeon(R) Scalable procesors A0/R0 are not supported starting 
    from BIOS R01.02.0001 (9535D03).   
12. BIOS R01.02.0003 contains the new secure boot components KEK and DB for Microsoft 2025.
    KEK – Microsoft Corporation KEK 2K Certificate Authority (CA) 2023*.
    DB – Windows UEFI CA 2023*, Microsoft UEFI CA 2023* and Microsoft Option ROM UEFI CA 2023*.
    Please be aware that new secure boot keys are necessary for Windows 2025. To update the new DB/KEK keys, previous secure boot keys stored in BIOS must be removed. The user must include the "UpdateNvram" parameter when flashing 
    BIOS R01.002.0003 image. 
13. User must add the parameter 'UpdateNvram' in the BIOS script before performing a firmware downgrade from R01.02.004 to lower versions; otherwise, TCC events may be recorded in SEL.

 Note: The "UpdateNvram" parameter will reset all previously configured BIOS settings to their default values


================================================================================
                                                      KNOWN ISSUES/WORKAROUND
================================================================================
1. Once the "Promote Warning" option is enabled, please do not use the Samsung
   Memory with date code WW34 2021.

2. On systems with 5th Gen Intel(R) Xeon(R) Scalable Processor and Compute
   Express Link (CXL) device installed, the "CPU C State Control" value must be
   set to "C0/C1 state" to disable "Package C State" support. Otherwise, the
   following Machine Check Timeouts may occur:

	MCA_IAL_TX_RUN_BUSY_TIMEOUT
	MCE_TOR_TIMEOUT

   The issue will be addressed in the future microcode release.
================================================================================
                                                      CHANGE LIST
================================================================================
		                R01.02.0006
================================================================================
1. Change BIOS ID to SE5C741.86B.01.02.0006.2605102119
2. PSIRT PTK0006547 An out-of-bounds read and write vulnerability in the BackupBiosUpdate.efi module may be exploited to allow SMRAM memory to be accessed and modified through an unvalidated firmware volume section header offset
3. Update CVE Fixes.
   2025-31648 (DocID: 860585)
   2025-35991 (DocID: 864913)
   2025-31944 (DocID: 862003)
   2025-27940 (DocID: 862003)
   2025-27572 (DocID: 862003)
   2025-32467 (DocID: 862003)
   2025-32007 (DocID: 862003)
   2025-30513 (DocID: 862003)
   2025-31356 (DocID: 868241)
4. PSIRT PTK0006073 - The usage is incorrect as “Varsize” should be used to indicate the size of data buffer, not the target variable size.
5. PSIRT PTK0006164 - “Size” should be initialized to the size of “CurrGetSetVarBuffer”. 
6. PSIRT PTK0006170 - Do a size check and Initialize Size.
7. PSIRT PTK0006166 - “VarSizeGe” should be initialized before set variable.
8. PSIRT PTK0006167 - “Size” should be initialized before set variable.
9. Copyright is changed to 2006-2026.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.116.D.10 (IPU26.2)
================================================================================
		                R01.02.0005
================================================================================
1. Change BIOS ID to SE5C741.86B.01.02.0005.2512081849
2. Renew MiTAC Root Key for ITK File
3. Update CVE Fixes.
   2025-20613 (DocID: 845725)
   2025-22853 (DocID: 845725)
   2025-21096 (DocID: 845725)
   2025-21090 (DocID: 845986)
   2025-24305 (DocID: 845986)
   2025-20053 (DocID: 845986)
   2025-20064 (DocID: 845456)
   2025-20068 (DocID: 845456)
   2025-20105 (DocID: 845456)
   2025-20028 (DocID: 845456)
   2025-20027 (DocID: 845456)
   2025-20073 (DocID: 845456)
   2025-22885 (DocID: 851350)
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.115.D.14 (IPU25.4)
================================================================================
		                R01.02.0004
================================================================================
1. Change BIOS ID to SE5C741.86B.01.02.0004.2506102329
2. CCB#4857 [BIOS] Expose 'Data Link Feature Exchange' in FCP/DNP BIOS SETUP Interface
3. Update CVE Fixes.
   2025-20054 (DocID: 838765)
   2025-20103 (DocID: 838765)
   2024-45332 (DocID: 838163)
   2025-20044 (DocID: 837145)
   2025-20109 (DocID: 837953)
4. Copyright is changed to 2006-2025.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.114.D.30 (IPU25.2)
================================================================================
		                R01.02.0003
================================================================================
1. Change BIOS ID to SE5C741.86B.01.02.0003.2412091841
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.113.D.55 (UPLR3)
================================================================================
		                9538.D02
================================================================================
1. PSIRT PTK0005244(CVE-2025-20034) - BackupBiosUpdate - Information disclosure vulnerability“DataSize” should be re-initialized before calling “SetVariable” in “CheckandUpdateBackupbootblock”.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.113.D.55 (UPLR3)
================================================================================
		                9538.D01
================================================================================
1. Update CVE Fixes.
   2024-31157 (DocID: 825181)
   2024-28047 (DocID: 825181)
   2024-39279 (DocID: 825181)
   2024-31068 (DocID: 823417)
   2024-37020 (DocID: 827347)
   2024-25571 (DocID: 827340)
   2024-21859 (DocID: 827463)
   2024-31155 (DocID: 827463)
   2024-26021 (DocID: 825068)
   2024-30211 (DocID: 825068)
   2024-36242 (DocID: 827909)
   2024-TBD   (DocID: 828378)
   2024-33607 (DocID: 826399)
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.113.D.55 (UPLR3)
================================================================================
		                9537.D01
================================================================================
1. PSIRT PTK0004953(CVE-2024-32050) - Certain DXE module BootOrderPolicyDxe whose GUID is 4F35CA6F-447A-40B3-AA01-7DE4EA1D1330 has a vulnerability
2. Add Microsoft new KEK and DB.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.111.D.23 (UPLR2 OOB)
================================================================================
		                R01.02.0002
================================================================================
1. Replace MiTAC Root Key for ITK File
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.109.D.34 (UPLR1 OOB)
================================================================================
		                9536.D05
================================================================================
1. PSIRT PTK0004845 GenerationSetup - Information disclosure vulnerability
2. PSIRT PTK0004850 OutOfBandXML - Information disclosure vulnerability
3. PSIRT PTK0004851 OutofBandFeature - Information disclosure vulnerability
4. PSIRT PTK0004856 When in SMM mode, the status of get variable is not checked
5. BTS: FCP#131, DNP#135 The Help text of "Correctable Error Threshold" needs to improve due to the default value changing.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.109.D.34 (UPLR1 OOB)
================================================================================
		                9536.D03
================================================================================
1. BTS: FCP#125, DNP#129 There is "Intel(R) Optane(TM) PMem Setting" page in servertool.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.109.D.34 (UPLR1)
================================================================================
		                9536.D01
================================================================================
1. PSIRT PTK0004706 Improper Input Validation in SmbiosOobMdr2 may result in information disclosure
2. PSIRT PTK0004531 Denali Park - SmiVariable driver: Intel Server SMM vulnerability
3. BTS: FCP#112 Slot Designation of SMBIOS type9 does not match silkscreen on RISER1_2U_1Slot_w/RT.
4. BTS: FCP#113 New DB to support Mitac key.
5. BTS: FCP#117 Expose CXL knobs to support CXL type 3 device.
6. CCB#4822 Add PRSCapability setup knob
7. CCB#4841 Change the default value for 'Correctable Error threshold' and 'Trigger SW Error Threshold'
8. Intel security advisories are already in this version as below.
   Intel-SA-01046, Intel-SA-01036, Intel-SA-01070, Intel-SA-01073, Intel-SA-01076, Intel-SA-01078
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.109.D.34 (UPLR1)
================================================================================
		                R01.02.0001
================================================================================
1. Change SVN number to 3
2. BIOS copyright date is updated to 2024
3. BTS: FCP#91, DNP#95 There is a CPU SMI time-out event after setting the new password via syscfg with the command syscfg    /bap (old password) (new password).
4. IPU 2024.1 SPR fixes included in this BIOS release: 
   [IPU2024.1]INTEL-SA-00972: Non-transparent sharing of return predictor targets between contexts in some Intel®       Processors may allow an authorized user to potentially enable information disclosure via local access.
   [IPU2024.1]INTEL-SA-00982: Trusted Execution Configuration Register Access
   [IPU2024.1]INTEL-SA-00960: Error Injection and Intel® Hyper-Threading  Disabled
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.107.D.52
================================================================================
		                9535.D05
================================================================================
1. BTS: DNP#86 "Signed Driver Check (CheckLogo)" test failed under windows server 2022
2. Add Two hot-fixes for Intel Known issue.
- Signed Driver (Logo) WHQL Test Will Fail on Device ACPI/INTC107F
- Production Intel SGX Attestation may fail on Emerald Rapids Production Samples
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.107.D.52
================================================================================
		                9535.D04
================================================================================
1. PSIRT PTK0004513 Stack buffer overflow leads to arbitrary code execution in a DXE driver 
2. PSIRT PTK0004533 PprRequestLog: Intel Server vulnerablility.
3. BTS: FCP#69, DNP#66 SUT is rebooting over and over with CPU Q3W6 after set SW Guard Extensions(SGX) to Enabled.
4. Correct the port mapping string for "TxEq Override mode" knobs in PCIe Misc. Configuration (Denali Pass)
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.107.D.52
================================================================================
		                9535.D03
================================================================================
1. PSIRT PTK0004402 The memory buffer used by “UserAuthenticationSmm.inf” is not checked.
2. PSIRT PTK0004403 DataSize needs to reinitialize for another GetVariable with different variable name.
3. PSIRT PTK0004480 Buffer needs to be checked before using.
4. CCB#4826 Add support for new VROC RAID Key
5. Add the ITK Key with the extended valid date.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.107.D.52
================================================================================
		                9534.D01
================================================================================
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.106.D.62
================================================================================
		                9533.D01
================================================================================
1. BTS: FCP#58 Support MiTAC Root Key for ITK File
2. Fix Coverity Issue ID2673702, Out-of-bounds access.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.105.D.74
================================================================================
		                9532.D02
================================================================================
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.105.D.48
================================================================================
		                9531.D01
================================================================================
1. CCB#4824  CPLD will trigger OBB timeout when updating RTM FW over 25 minutes.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.105.D.20
================================================================================
		                9530.D02
================================================================================
1. BTS: FCP#27, DNP#31 Can't Boot to Windows 2022 correctly with EMR CPU Q2SR
2. BTS: FCP#34 Memory Speed Selection up to 5600.
3. BTS: FCP#38, DNP#35 The Active Processor Cores can't be set to above 55 cores.
4. BTS: FCP#41 Link width of Intel OCP3.0 E810-CQDA2 is x4 on FCP.
5. BTS: FCP#40, DNP#36 There is no an error of variable reclaimed on Error Manager of BIOS Setup after do "Reboot SUT" by command "reset" on UEFI Internal Shell with CPU CPU Q2SR.
6. BTS: FCP#42, DNP#37 The Patrol scrub register isn’t 1 when Patrol scrub is set to Enable at the End of POST.
7. BTS: FCP#44 SUT will halt at 0x07 after flashing BIOS 9528D04_SPRSDP_dev.
8. CCB#3670 Need ability to clear and change BIOS admin password over Redfish.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.104.D.47
================================================================================
		                9529.D01
================================================================================
1. BTS: FCP#26, DNP#30 There is one Yellow Mark in Windows 2022 with EMR CPU.
2. BTS: FCP#31 Add TxEq items in GenerationSdpConfiguration to control TxEq settings when build SDP BIOS
3. BTS: FCP#30 "HW Validation Test only" is present in BIOS Setup Menu
4. BTS: FCP#29 UPI speed is unknown.
5. Hsd-es: 15012997376 Remove PMEM Items from EGS BIOS.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.104.D.25
================================================================================
		                9528.D04
================================================================================
1. Hsd-es: 2103658030 Riser2 interposer bifurcation doesn't change to x8x4x4 on ITP after setting Riser2_Slot2 Bifurcation to <x8x4x4> via Setup UI.
2. Hsd-es: 15013347473 On Denali Pass, Redfish Host Interface name can't be found in /sys/bus/usb/devices in SLES 15 SP4
3. Hsd-es: 22017955759 Setting bifurcation to x2 in BIOS shows as x4 instead
4. Hsd-es: 14019090517 Enable Reserved Memory Reporting (RMRR) in FCP BIOS
5. Hsd-es: 22018204723 System BIOS set to 1LM but booting HBM memory in 2LM mode.
6. Hsd-es: 2103654782 There is "PCIeCorrectableReceiverError" redfish event with LC OAM SKU during power cycling test
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.103.D.42
This release is base on SPR 9525D25.
================================================================================
		                R01.01.0005
================================================================================
1. Hsd-es: NA [DSG]Change BIOS ID to SE5C741.86B.01.01.0005
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.28
================================================================================
		                9525.D25
================================================================================
1. Hsd-es: 2103657758 [DSG]Hide C1E when Optimized Power Mode set to Enabled
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.28
================================================================================
		                9525.D24
================================================================================
1. Hsd-es: 15012814795 [DSG][Redfish]Some values of some BIOS registration attributes does not match the actual situation.
2. Hsd-es: 15013075175 [DSG]SMBIOS type 17 of disabled DIMM show incorrect AssetTag
3. Hsd-es: 15013124284 [DSG] Check PPR repair status before log SEL
4. Hsd-es: 2103657719 [DSG] DDR5 PPR variable data has been cleared on HBM sku.
5. Hsd-es: 15013038846 [DSG]Align IFWI id and Work Week time zone to local time zone.
6. Hsd-es: 15013050836 [DSG]Change "ITK" to "BIOS" in Clear Setting message
7. Hsd-es: NA [DSG]Align Errorcode Message with EPS
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.28
================================================================================
		                R01.01.0004
================================================================================
1. Hsd-es: NA [DSG] Change BIOS ID to SE5C741.86B.01.01.0004
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.28
================================================================================
		                9525.D21
================================================================================
1. Hsd-es: NA [DSG]Fix processor information display error cased by pr39684
2. Hsd-es: 15013015241 [DSG] Fix incorrect 8501 and 8502 error code caused by "WARN_DIMM_NOT_IN_DDRT_POR_DDR_TABLE".
3. Hsd-es: 15013024551 [DSG] CPLD WD Reset for Retimer Update for SDP only
4. Hsd-es: 2103655983 [DSG] CPLD will trigger OBB timeout when updating RTM FW over 25 minutes.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.28
================================================================================
		                9525.D18
================================================================================
1. Hsd-es: NA [DSG]Add VrocSwLicense Driver
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.28
================================================================================
		                9525.D17
================================================================================
1. Hsd-es: NA DSG EGS-SPR Reduced UMA Based clustering modes per EGS population
2. Hsd-es: 16019805833 [DSG] System Fails to boot with specific set of knobs changes from ITK
3. Hsd-es: 15012705004 [DSG] Enhance SMBIOS Type 9 to support multiple PCI root port within the same slot
4. Hsd-es: 15012878351 [DSG] Update BIOS Splash Screen file on DSG FCP/DNP.
5. Hsd-es: 22016516982 [DSG] Expose "C1 Auto Demotion" in ITK
6. Hsd-es: NA [DSG] Code Sync to IFWI 2023.07.2.03 Orange Release BIOS 9409.P28
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.28
================================================================================
		                R01.01.0003
================================================================================
1. Hsd-es: NA [DSG] Change BIOS ID to SE5C741.86B.01.01.0003.2302100643.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.15
================================================================================
	                        9525.D13
================================================================================
1. Hsd-es: 15012733428 [DSG] Remove Enforced Password Support knob
2. Hsd-es: 15012714739 [DSG] Update NTB knob name to align with RP
3. Hsd-es: NA [DSG] Code Sync to IFWI 2023.03.2.04 Orange Release BIOS 9409.P15
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.15
================================================================================
		                9525.D09
================================================================================
1. Hsd-es: 15012673050 [DSG] Update ITK root cert which is provided by utility
   team in HSD 16018908440
2. Hsd-es: 15012637059 [DSG] Remove PCIe PLL SSC knob following RP change
3. Hsd-es: 22016516982 [DSG] Expose C1 Auto Demotion knob in CPU C State page
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.95.D.25
================================================================================
		                9525.D07
================================================================================
1. Hsd-es: N/A [DSG]Remove "RAID Mode" option from "ACHI Capable SATA Controller" knob.
2. Hsd-es: 2103656811 [DSG] Add a workaround to fix SMBIOS Type190 can not get E810-CQDA2 NIC card slod number
3. Hsd-es: 15012367393 [DSG] Add Optimized Power Mode knob
4. Hsd-es: N/A [DSG] Ignore UefiDrivers folder and ApiDrivers folder.
5. Hsd-es: 2103656955 [DSG] Slot ID mismatch silkscreen of RISER1_2U_1Slot_w/RT on FCP
6. Hsd-es: N/A [DSG][CCB3746] Add FCP SDP ME SPS xml build for CCB3746 test BIOS
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.95.D.25
================================================================================
		                9525.D03
================================================================================
1. Hsd-es: N/A [DSG] Suppress SNC4 for SPR MCC/LCC
2. Hsd-es: 15012360420 [DSG] Help text of PMem FastGo Configuration does not match
3. Hsd-es: N/A [DSG] BIOS copyright should change to 2006-2023
4. Hsd-es: 2103656878 [DSG] Fix the issue that HBM isn't in cache mode after setting HBM Mode to 2LM with 4+0 or 8+0 configuration.
5. Hsd-es: 14018275036 [DSG] Remove "RAID Mode" option from "ACHI Capable SATA Controller" knob.
6. Hsd-es: N/A [DSG] Code Sync to IFWI WW52 Orange Release 95D25.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.95.D.25
================================================================================
		                9409.D04
================================================================================
1. Hsd-es: N/A [DSG] Remove "SATA" and "SSATA" string from VMD page.
2. Hsd-es: 15012255060 [DSG] [SDP] [CCB3746] Use RP IOU Bifurcation knobs in IOU Configuration for FCP SDP BIOS
3. Hsd-es: 15011965130 [DSG] Automatically detect bios id instead of detecting by hardcode in IFWIingredienttable html.
4. Hsd-es: 15012499353 [DSG] Remove GenerationID variable due to not used.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.01
================================================================================
		                R01.01.0002
================================================================================
1. Hsd-es: NA [DSG]Change BIOS ID to SE5C741.86B.01.01.0002.2212220608.
================================================================================
		                9409.D03
================================================================================
1. Hsd-es: N/A [DSG] New knob HBM Mode for SPR-HBM
2. Hsd-es: 15012493889 [DSG] Remove Auto info of BIOS knobs Attempt Fast Boot & Attempt Fast Cold Boot
3. Hsd-es: 15012333630 [DSG] Support Test BIOS Build and Factory BIOS Build
4. Hsd-es: N/A [DSG] Change Volatile Memory Mode default vaule from 2LM to 1LM for SPR-SP.
5. Hsd-es: 15012360420 [DSG] Mismatch help info between UG and Setup UI.
6. Hsd-es: 2103655451 [DSG] XmlCli build script can not parse bios knob dependency with NOT expression correctly
7. Hsd-es: 15012232086 [DSG] fix SGX HII info for POR memory population
8. Hsd-es: 2103655434 [DSG] TME value is not consistent between BIOS and Redfish after modifying it
9. Hsd-es: N/A [DSG] Code Sync to IFWI WW49 Orange Release 9409P01
10. Hsd-es: 15012255060 [DSG] [CCB3746] Add two debug knob to SDP BIOS for CCB3746 test BIOS.
11. Hsd-es: 2103656524 [DSG] Bypass HBM channel when check channel number
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.9409.P.01
================================================================================
		                9223.D04
================================================================================
1. Hsd-es: 15012154290 [DSG] HW validation Page knobs cleanup for SDP BIOS
2. Hsd-es: 2103656200 [DSG] Clear IP address, subnetmask and gateway to zero when change IP mode from dynamic to static
3. Hsd-es: 2103655646 [DSG] Do workaround since BMC can not recognize the priority of AND and OR
4. Hsd-es: 15012276490 [DSG] Attempt fast boot / Attempt fast cold boot option value will be overwritten to enable after online update
5. Hsd-es: N/A [DSG] BMC IP address will not be cleared if set IP resource form dynamic to static
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.92.D.23
================================================================================
		                9223.D02
================================================================================
1. Hsd-es: 15012278262 [DSG] Add Allow Memory Test Correctable Error knob to Memory Configuration page
2. Hsd-es: 2103656039 [DSG] Hide "Intel SST-PP" from ITK
3. Hsd-es: 15012255060 [DSG] Without any UPI CE EWS event after the first injected UPI correctable error
4. Hsd-es: NA [DSG] Change SDP BIOS PFR default value back to unlocked.
5. Hsd-es: 2103656343 [DSG] Send “SET_FAN_PROFILE” command when dimm installed or CPU is HBM CPU
6. Hsd-es: NA [DSG] Code Sync to IFWI WW46 Orange Release 92D23
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.92.D.23
================================================================================
		                9105.D05 / R01.01.0001
================================================================================
1. Hsd-es: NA [DSG]Change SVN is 2
2. Hsd-es: NA [DSG]Enable PFR lock by default
3. Hsd-es: 15012278088 [DSG] Integrate HBM AMT Knobs from Reference Code
4. Hsd-es: 15012255060 [DSG] [CCB3746] Add knob "PCI AER Support" to SDP BIOS for CCB3745 test BIOS.
5. Hsd-es: NA [DSG]Change BIOS ID is SE5C741.86B.01.01.0001.xxxxxxxx(timestamp)
6. Hsd-es: NA [DSG]Add warning message of factory build.
This release is mapping to RP release Reference code version: EGLSTRM.0.RPB.91.D.05
===============================================================================
REFERENCE MATERIAL
===============================================================================

[Intel® Server Board D50DNP and M50FCP Family BIOS Setup Utility User Guide]
https://www.intel.com/content/www/us/en/content-details/733108/content-details.html
